1. LISTING
	1. UL (UL508A – Industrial Pump Controllers)
2. MANUFACTURER AND MODEL
	1. Tornatech Inc. model DSM
3. SUPERVISORY POWER
	1. 120V / 1ph / 60Hz

1. FIELD CONNECTION FOR EXTERNAL DEVICES
	1. Provision to connect stop fill fuel level float switch

1. ENCLOSURE
	1. NEMA 4x vandal-proof, dead front fiberglass
	2. Wall mounting lugs (x4)
	3. Padlockable snap latch
	4. Inner door
	5. Anti-condensation thermostat and space heater
2. VISUAL INDICATORS AND OPERATORS
	1. Test / Silence selector switch
	2. Stop Fill pilot light
	3. Supervisory Power ON pilot light
3. AUDIBLE ALARM
	1. Alarm horn rated for 100dB at 10ft (3m)