1. LISTING
   1. UL (UL508A – Industrial Pump Controllers)
2. MANUFACTURER AND MODEL
   1. Tornatech Inc. model DSM
3. SUPERVISORY POWER
   1. 120V / 1ph / 60Hz

1. FIELD CONNECTION FOR EXTERNAL DEVICES
   1. Provision to connect stop fill fuel level float switch

1. ENCLOSURE
   1. NEMA 4x vandal-proof, dead front fiberglass
   2. Wall mounting lugs (x4)
   3. Padlockable snap latch
   4. Inner door
   5. Anti-condensation thermostat and space heater
2. VISUAL INDICATORS AND OPERATORS
   1. Test / Silence selector switch
   2. Stop Fill pilot light
   3. Supervisory Power ON pilot light
3. AUDIBLE ALARM
   1. Alarm horn rated for 100dB at 10ft (3m)