1. Certifications
2. CE Mark
3. MANUFACTURER AND MODEL
	* 1. Tornatech model JFY
4. OPERATIONAL COMPONENTS AND STARTING METHOD
5. Combined manual and automatic
6. Horsepower rated disconnect switch
7. Wye delta open starter
8. Thermo-magnetic motor protector
9. Transformer with 24V.AC secondary
10. ENCLOSURE
11. IP55
12. OPERATOR INTERFACE
13. Touch-pad type pushbuttons and a high luminosity LED digital display.
14. Shall monitor and display motor operating conditions and pressure conditions
15. Operational without opening the controller door.
16. VISUAL INDICATIONS
17. The operator interface shall indicate:
18. Manual motor run LED
19. Automatic motor run LED
20. Motor overload
21. System pressure
22. Start pressure
23. Stop pressure
24. System pressure above stop pressure LED
25. System pressure in between start and stop pressure LED
26. System pressure below start pressure LED
27. Controller in AUTO mode
28. Controller in OFF mode
29. Pump start counter
30. Elapsed time meter (hours / non-resettable)
31. TIMERS
32. Minimum run period timer
33. Sequential start timer.
34. SOLID STATE PRESSURE TRANSDUCER
35. Stainless steel
36. Operational between 0 and 600psi
37. External connection