1. APPROVALS
2. UL508A
3. MANUFACTURER AND MODEL
4. Tornatech model JPLT
5. OPERATIONAL COMPONENTS AND STARTING METHOD
6. Combined manual and automatic
7. Type-F fuse-less magnetic motor starter
8. Main disconnect handle
9. HAND-OFF-AUTO pushbuttons
10. MENU navigation pushbuttons
11. ENCLOSURE
12. NEMA Type 2
13. OPERATOR INTERFACE
14. Touch-pad type pushbuttons and a high luminosity alphanumeric display.
15. Shall monitor and display motor operating conditions and system pressure conditions
16. Operational without opening the controller door.
17. VISUAL INDICATIONS
18. H-O-A position
19. System pressure
	1. Adjustable in PSI, BAR
20. Cut-out and Cut-In pressure setting
21. Manual motor run
22. Automatic motor run
23. Motor overload (occured)
24. Pump start counter
25. Elapsed time meter (hours / non-resettable)
26. Audible alarm
27. TIMERS
28. Minimum run period timer
29. Sequential start timer.
30. SOLID STATE PRESSURE TRANSDUCER
31. Stainless steel
32. Operational between 0 and 600psi
33. External connection